// File: rm18f14k50_g.lkr
// Linker script for the PIC18F14K50 processor, with some modifications to allow
// the output .hex file to be programmable with the HID USB bootloader.  This linker
// file is intended to be used with "application" projects (not the bootloader firmware
// project itself).

#DEFINE _CODEEND _DEBUGCODESTART - 1
#DEFINE _CEND _CODEEND + _DEBUGCODELEN
#DEFINE _DATAEND _DEBUGDATASTART - 1
#DEFINE _DEND _DATAEND + _DEBUGDATALEN

LIBPATH .

#IFDEF _CRUNTIME
  #IFDEF _EXTENDEDMODE
    FILES c018i_e.o
    FILES clib_e.lib
    FILES p18f14k50_e.lib

  #ELSE
    FILES c018i.o
    FILES clib.lib
    FILES p18f14k50.lib
  #FI

#FI

CODEPAGE   NAME=bootloader START=0x0               END=0xFFF        PROTECTED
CODEPAGE   NAME=boot_vec   START=0x1000            END=0x101F       PROTECTED
#IFDEF _DEBUGCODESTART
  CODEPAGE   NAME=page       START=0x1020            END=_CODEEND
  CODEPAGE   NAME=debug      START=_DEBUGCODESTART   END=_CEND        PROTECTED
#ELSE
  CODEPAGE   NAME=page       START=0x1020           END=0x3FFF
#FI

CODEPAGE   NAME=idlocs     START=0x200000          END=0x200007       PROTECTED
CODEPAGE   NAME=config     START=0x300000          END=0x30000D       PROTECTED
CODEPAGE   NAME=devid      START=0x3FFFFE          END=0x3FFFFF       PROTECTED
CODEPAGE   NAME=eedata     START=0xF00000          END=0xF000FF       PROTECTED

#IFDEF _EXTENDEDMODE
  DATABANK   NAME=gpre       START=0x0               END=0x5F
#ELSE
  ACCESSBANK NAME=accessram  START=0x0               END=0x5F
#FI

DATABANK   NAME=gpr0       START=0x60              END=0xFF

#IFDEF _DEBUGDATASTART
  DATABANK   NAME=gpr1       START=0x100             END=_DATAEND
  DATABANK   NAME=dbgspr     START=_DEBUGDATASTART   END=_DEND           PROTECTED
#ELSE //no debug
  DATABANK   NAME=gpr1       START=0x100             END=0x1FF
#FI

DATABANK   NAME=usb2       START=0x200             END=0x2FF
DATABANK   NAME=sfr15      START=0xF53             END=0xF5F          PROTECTED
ACCESSBANK NAME=accesssfr  START=0xF60             END=0xFFF          PROTECTED

#IFDEF _CRUNTIME
  SECTION    NAME=CONFIG     ROM=config
  #IFDEF _DEBUGDATASTART
    STACK SIZE=0x60 RAM=gpr0
  #ELSE
    STACK SIZE=0x60 RAM=gpr1
  #FI
#FI

SECTION    NAME=usbram2     RAM=usb2
SECTION    NAME=USB_VARS   RAM=usb2
